Added to Your
Shopping Cart
text.skipToContent text.skipToNavigation

#

5

Browse 104 results for "2-0"

Showing

30

of 104 results
FILTER & SORT
Sort by:
Compare Products Compare Series
View:
Filter Results Results refresh instantly as you filter.
Category

###### Filter by Category

Our products, brands, and resources fall under many unique categories based on the product's type or function. Filter and find a product you are looking for based on a Legrand product category.

- Lighting Controls and Systems (5)
  - Power Packs and Load Controllers (5)
    - Room Controllers (3)
    - In-Fixture Controllers (2)
  - Digital Lighting Management (3)
    - Load Controllers (3)
  - Occupancy and Vacancy Sensors (2)
    - In-Fixture Sensors (2)
- Wiring Devices (2)
  - Designer Switches and Outlets (1)
    - Dimmers (1)
  - Light Switches and Dimmers (1)
    - Dimmers (1)
  - radiant Collection (1)
    - Dimmers (1)
  - Plugs and Connectors (1)
    - Cam Type Devices (1)
- Wire and Cable Management (1)
  - Branch Circuit Wiring (1)
    - Wall Box Mounting Components (1)

Brand

###### Brand

Choose from one of Legrand's brands.

- Wattstopper (5)
- radiant Collection (1)
- Cablofil (1)
- Pass and Seymour (1)

Sensor Type

###### Sensor Type

The Device that Receives a Signal or Stimulus (As Heat or Pressure or Light or Motion Etc.) and Responds to it in a Distinctive Manner

- Daylight (2)
- Occupancy (2)

Installation Location

###### Installation Location

Where a Device is or is to be Installed

- Pole (1)
- Ceiling (3)
- Fixture (1)

NEMA Rating

###### NEMA Rating

National Electrical Manufacturers Association Ratings are Standards that are Useful in Defining the Types of Environments in Which an Electrical Enclosure can be Used

- WD 7 (2)

Availability

###### Availability

Product is available to buy on Legrand.us

- Get it online (1)

Compatibility

###### Compatibility

Capability of Being Used with or Connected to Different Types of Devices or Components without any Modifications

- Bluetooth (2)
- DLM Wired (3)

Certifications

###### Product Certifications

Trust in quality and compliance. Use this filter to find products that have undergone thorough testing and evaluation to ensure they meet the quality and safety standards for a wide range of certifications.

- BAA Compliant (3)
- CSA Listed (1)
- cULus Listed (1)
- DLC Listed (4)
- ioXt Certified (4)
- PEP (3)
- RoHS Compliant (5)

- BAA Compliant (3)
- CSA Listed (1)
- cULus Listed (1)
- DLC Listed (4)
- ioXt Certified (4)
- PEP (3)
- RoHS Compliant (5)
- UL Listed (2)
- WELL Building Standard (1)

SHOW MORE SHOW LESS
Frequency Rating

###### Frequency Rating

The Number of Occurrences within a Given Time Period, the Rate at Which Alternating Current Makes a Complete Cycle of Reversals

- 60 Hz (1)

Indoor/Outdoor

###### Indoor/Outdoor

Enviromental Conditions rating on the product. Indoor Only, Outdoor, Both

- Both (2)
- Indoor (4)

Type

###### Type

Value that Specifically Names the Type/the Application Value of the Closest Piece of Equipment/the Designated Type of Construction/the Generic Type/the Manufacturer Type Designation/the Specific Function/the Type of Application

- Sensor (2)
- Room Controller (3)
- Dimmer (1)

Timer Duration

###### Timer Duration

Amount of Time a Timer can Last

- 30 Seconds, 5-30 Minutes (2)

Input Voltage

###### Input Voltage

The Difference of Electrical Potential Between Two Points of an Electrical or Electronic Circuit Entering a System

- 12 to 32 VDC (2)
- 120/277 VAC (2)
- 120/230/240/277 VAC (1)
- 347 VAC (1)

Load Type

###### Load Type

Denotes the type(s) of load that can be applied to a dimmer, which determines its compatible light sources.

- Fluorescent (1)

Output Voltage

###### Output Voltage

The Voltage Measured at the Output Terminals of a Power Supply

- 24 VDC (3)

Mounting Type

###### Mounting Type

The way the item is mounted for display. The method by which a sign or label is affixed to a surface for display. Many signs will not have any defined mounting type and so will have no value captured for this attribute.

- Fixture Embedded (2)
- Drop Nipple (1)
- Wall Box (1)
- Threaded Collar (1)
- 1/2 in Knockout (2)
- 4 in Deep J-Box (3)

Has Battery

###### Has Battery

A Device for Converting Chemical Energy Into Electrical Energy a Group of Two or More Connected Voltaic Cells

- No (5)

Wire Size

###### Wire Size

It is the Normal Size of the Conductors for Building Wire

- #14 - #10 AWG (1)

Load Rating

###### Load Rating

The maximum load that a device is designed to withstand without breakage or loss of performance.

- 120V 8A (Fluorescent) (1)

Color

###### Color

The color of the product itself

- White (6)
- Black (1)
- Bronze (1)
- Gray (1)
- Ivory (1)
- Light Almond (1)

Sensing Range

###### Sensing Range

The total Possible Sensing Capability of the Sensor, Beginning After the Deadband, and Extending Out as Far as the Sensor is Able to Reach Effectively

- 40 ft diameter (1)
- 44 ft diameter (1)
- 100 ft diameter (1)

Number of Switches

###### Number of Switches

Number of electrical switches

- 1 (1)

Voltage

###### Voltage

The Rate at Which Energy is Drawn from a Source that Produces a Flow of Electricity in a Circuit

- 120 VAC (1)

Operating Temperature

###### Operating Temperature

The Temperature at Which the Unit is Safely Operated or Kept without Damaging or Changing the performance Characteristics of the Unit

- 0°-55°C (2)
- 0°-70°C (1)
- 0°-60°C (1)
- 32°-131°F (2)
- 32°-158°F (1)
- 32°-140°F (1)
- -40°-167°F (2)

- 0°-55°C (2)
- 0°-70°C (1)
- 0°-60°C (1)
- 32°-131°F (2)
- 32°-158°F (1)
- 32°-140°F (1)
- -40°-167°F (2)
- -40°-75°C (2)

SHOW MORE SHOW LESS
Included

###### Included

The Supplementary items Supplied with the Product Which May be Necessary for the Optimum Operation of the Product

- Collar (1)

Product Width

###### Product Width

The overall width of the product.

- 2.25 in (1)
- 2.3 in (1)
- 2.5 in (1)
- 3.9 in (1)
- 4.0 in (1)
- 4.147 in (1)
- 5.818 in (1)

- 2.25 in (1)
- 2.3 in (1)
- 2.5 in (1)
- 3.9 in (1)
- 4.0 in (1)
- 4.147 in (1)
- 5.818 in (1)
- 6.235 in (1)
- 6.5 in (1)

SHOW MORE SHOW LESS
Wire Connection Type

###### Wire Connection Type

Describes the method used to connect wires to the device, such as screw terminals, push-in connectors, or lead wires.

- RJ-45 (3)
- Terminal Block (3)
- Flying Leads (2)
- Screw Terminals (1)

Preset

###### Preset

Denotes whether a dimmer returns lights to their previously-selected light level when turned on.

- Yes (1)

Operating Temperature Min

###### Operating Temperature Min

Indicates the lowest possible temperature a device can be safely used without the risk of failure or damage.

- 32.0 °F (3)
- -40.0 °F (2)

On Function

###### On Function

Describes the mode of operation for devices that can be turned on, indicating whether they stay on continuously or operate on a timer or sensor.

- Auto On (2)

Number of Connections

###### Number of Connections

The number of connections a product is able to make to other devices.

- 4.0 (2)
- 7.0 (1)

Standard

###### Standard

The industrial standard(s) to which a device is manufactured, operated, or tested.

- cUL (5)
- FCC part 15 (3)
- ISO 14001 (3)
- ISO 14025:2010 (3)
- PEP (3)
- RoHS 2011/65/EC (3)
- UL 2043 (3)

- cUL (5)
- FCC part 15 (3)
- ISO 14001 (3)
- ISO 14025:2010 (3)
- PEP (3)
- RoHS 2011/65/EC (3)
- UL 2043 (3)
- UL 60730 (3)
- UL 924 (3)
- BAA (3)
- TAA (3)
- CE (2)
- E101196 (2)
- IP66 Rated (2)
- RoHS (2)
- UL (2)
- UL Listed (2)
- ISO 14040:2006 (1)
- ISO 14044:2006 (1)
- CSA Listed (1)
- cULus (1)

SHOW MORE SHOW LESS
Storage Temperature

###### Storage Temperature

Describes the temperature or range of temperatures at which a product can be safely stored or kept without damaging or altering the performance characteristics of the device.

- 23° - 176° F (3)
- -40° - 176° F (2)
- -40° - 80° C (2)

Indicator

###### Indicator

Describes the type/specification of signaling a device uses to indicate abnormal and/or operating conditions.

- PIR Detection LED (2)

Timer Type

###### Timer Type

The mechanism by which the timer operates, such as mechanical, digital, or programmable.

- Digital (2)

Dimming Compatibility

###### Dimming Compatibility

Describes the method(s) used by a device or system to adjust the brightness of a lighting load.

- 0-10 V (3)
- Forward Phase (1)

Application Sector

###### Application Sector

Refers to the expected environment(s) or intended usage(s) for a product (e.g. Residential, Commercial, Industrial, etc.).

- Commercial (6)
- Hospitality (1)
- Residential (1)

Product Depth

###### Product Depth

The overall depth of a product.

- 1.25 in (1)
- 2.0 in (2)
- 2.317 in (1)
- 2.419 in (1)
- 3.3 in (1)
- 3.667 in (1)

Topology

###### Topology

The arrangement in which the Nodes of a LAN are connected to each other.

- Free Topology (3)

Sensor Coverage Pattern

###### Sensor Coverage Pattern

Describes the shape of the area that a sensor is able to detect presence or movement within, measured in degrees.

- 360.0 ° (1)

Current Draw

###### Current Draw

The amount of electrical current the device uses during operation, measured in amperes (or amps).

- 10.0 A (2)
- 15.0 mA (2)
- 15.0 A (1)
- 20.0 A (1)

Requires Neutral Wire

###### Requires Neutral Wire

Indicates whether a device requires a neutral wire to function properly.

- No (1)

Operating Humidity

###### Operating Humidity

Describes the range of humidity at which a device can be utilized safely without the risk of failure or damage.

- 5-95% RH (Non-Condensing) (5)

Product Series

###### Product Series

A collection of related products that share a common design, technology, or purpose. Products within the series either maintain a cohesive brand / style identity or work together to serve a particular solution.

- LMRC (3)
- FSP-3x1B (2)

Country of Origin

- China (7)
- United States (3)
- Mexico (1)

Product Height

###### Product Height

The overall height of a product.

- 1.922 in (1)
- 2.8 in (1)
- 4.058 in (1)
- 4.0 in (1)
- 4.28 in (1)
- 4.25 in (1)
- 4.4 in (1)

- 1.922 in (1)
- 2.8 in (1)
- 4.058 in (1)
- 4.0 in (1)
- 4.28 in (1)
- 4.25 in (1)
- 4.4 in (1)
- 6.5 in (1)

SHOW MORE SHOW LESS
Switch Type

###### Switch Type

Refers to the style or operation method used by a switch to control lighting or other electrical devices.

- Paddle (1)
- Slider (1)

Line Frequency

###### Line Frequency

The frequency of alternating current (AC) in an electrical power system, measured in Hz. Also commonly referred to as Utility Frequency, Power Line Frequency, or Mains Frequency.

- 50.0 Hz (3)
- 60.0 Hz (3)

Maximum Humidity

###### Maximum Humidity

The highest level of atmospheric moisture a device can withstand without compromising functionality or safety.

- 90% (relative humidity, non-condensing) (1)

Features

###### Features

Unique characteristics and functionality that set the product apart from others in its field.

- Adjustable Time Delay (2)
- Flame Retardant (2)
- Impact Resistant (2)
- Light Level Sensor (2)
- Recyclable (2)
- Sensitivity Adjustment (2)
- UV Resistant (2)

- Adjustable Time Delay (2)
- Flame Retardant (2)
- Impact Resistant (2)
- Light Level Sensor (2)
- Recyclable (2)
- Sensitivity Adjustment (2)
- UV Resistant (2)
- Color Change Kit (1)
- Locator Light (1)
- Low-End Trim (Dim Range) (1)
- Metered (1)

SHOW MORE SHOW LESS
Sensor Technology

###### Sensor Technology

The technology used by a device to sense a change in signal or stimulus.

- Passive Infrared (PIR) (2)
- Photosensor (2)

Number of Poles

###### Number of Poles

Single pole switches have two terminals and control one light fixture from one location. 3-Way switches have three terminals and can control one fixture from two locations. 4-Way switches have four terminals can control one fixture from three locations. Multi-location refers to switches connected to a smart lighting system.

- Single Pole 3-Way (1)

Operating Temperature Max

###### Operating Temperature Max

Indicates the highest possible temperature a device can be safely used without the risk of failure or damage.

- 167.0 °F (2)
- 158.0 °F (1)
- 140.0 °F (1)
- 131.0 °F (2)

Warranty Type

###### Warranty Type

The product warranty that accompanies the specific product.

- 5-Year (5)
- Limited Lifetime Warranty (1)

Environmental Conditions

###### Environmental Conditions

Describes the relative range of climatic standards a device can safely operate within.

- Humidity: Less than 95% non condensing (1)

Finish

###### Finish

Describes the specific surface treatment applied to the outer product for either aesthetics and/or durability.

- Gloss (5)
- Pre-Galvanized (1)
- Satin (1)

Product Length

###### Product Length

The overall length of a product.

- 5.7 in (1)

Sensor Mounting Height

###### Sensor Mounting Height

Describes the optimal vertical distance at which a sensor should be installed to ensure reliable detection of motion or other target conditions.

- 40 ft (1)
- 20 ft (1)
- 8 ft (1)

Location Rating

###### Location Rating

Denotes the classification used to assess the suitability or performance of a device based on the specific environmental location in which it operates.

- Dry (3)
- Wet (2)

Number of Relays

###### Number of Relays

Denotes the number of controlled loads a device can support.

- 2.0 (3)

Material

###### Material

Indicates the primary material(s) used to construct a product.

- Polycarbonate (4)
- ABS (1)
- Steel (1)
- Thermoplastic (1)

Stock Level

###### Stock Level

Filter your results to only in-stock products sold directly on legrand.us.

- Out Of Stock (8)

FILTER & SORT
Sort by:
Compare Products
View:
Brand

###### Brand

Choose from one of Legrand's brands.

- adorne Collection (2)
- Legrand (2)
- Pass and Seymour (2)
- radiant Collection (2)
- Wattstopper (7)
- Wiring Devices (2)

Category

###### Category

Our brands, products, resources, and pages are group into divisions. Filter and find a product, resource, or page you are looking for based on a Legrand category.

- EV Chargers (2)
- Home EV Chargers (2)
- Smart Lighting (2)
- Wire and Cable Management (2)
- Wiring Devices (2)

FILTER & SORT
Sort by:
Compare Products
View:

- 1(current)
- 2
- 3

Product Category

###### Filter by Product Category

Filter downloadable resources by the product category they relate or are relevant to.

- Wire and Cable Management (76)
  - In-Floor Systems (76)
    - Distribution and Feeder Systems (76)
    - Service Fittings (5)
  - Poles and Columns (2)
    - Tele-Power Pole Extenders (2)

Brand

###### Brand

Choose from one of Legrand's brands.

- Wiremold (77)

Resource Type

###### Resource Type

Filter for different types of resources like CAD drawings, BIM objects, guide form specs, online configurators, white papers, brochures, or product cut sheets.

- BIM Models (12)
- Brochure (2)
- CAD Drawings (36)
- Catalog (1)
- Guide Form Specifications (2)
- Installation Instructions (2)
- Instruction Sheet (20)

- BIM Models (12)
- Brochure (2)
- CAD Drawings (36)
- Catalog (1)
- Guide Form Specifications (2)
- Installation Instructions (2)
- Instruction Sheet (20)
- Supporting Document (1)
- White Papers & Tech Bulletins (1)

SHOW MORE SHOW LESS
File Size

###### File Size

Filter downloadable resources by their approximate file size.

- < 1MB (75)
- 1MB to 2MB (1)
- > 8MB (1)

8 Products available
Sort by:
Compare Products Compare Series
View:

- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  DLM Room Controller, 2 Relay, 0-10V Dimming
  LMRC-212 Wattstopper
  LMRC-210 Series Digital Room Controllers include one, two or three relay(s) to switch a total of 15 or 20 amps, a highefficiency switching power supply and one 0-10 volt output per relay for control of dimmable loads including electronic ballasts (Advance Mark 7, or equivalent).

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  Other Options Available
  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  3-0 Round Adj.3/4'' - 1 1/2'' Plaster Ring Box Of 25 [Fp211054]
  APR-R Cablofil
  FASPower branch circuit wiring products dramatically reduce labor and increase productivity on the jobsite

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  45 DEG M CAM 2/0-4/0 SS PNL MT BL
  PS45MRBBL Pass and Seymour
  45 DEG M CAM 2/0-4/0 SS PNL MT BL

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  radiant® 2-Wire Fluorescent Dimmer, White
  RHFB83PW radiant Collection
  Delivers precise light level control with classic style

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  $61.77
  Out of stock on Legrand.us
  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  0-10V PIR FIXTURE SENSOR BLE 1 2-32V
  FSP-301B Wattstopper
  The FSP-3x1B sensors provide continuous dimming light level control based on motion and/or daylight contribution.

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  DLM Room Controller, 2 Relay, 0-10V, 10A, Metered, USA
  LMRC-112-M-U Wattstopper
  LMRC-110 series room controllers include one or two relay(s) to switch a total of 10 amps, a high-efficiency switching power supply and dual 0-10 volt outputs per relay for control of dimmable loads including compatible LED drivers or electronic ballasts. T

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  Other Options Available
  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  DLM Room Controller, 2 Relay, KO, 0-10V dimming, 10A
  LMRC-112 Wattstopper
  LMRC-110 series room controllers include one or two relay(s) to switch a total of 10 amps, a high-efficiency switching power supply and dual 0-10 volt outputs per relay for control of dimmable loads including compatible LED drivers or electronic ballasts.

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  Other Options Available
  View Details
- Favorite
  Added to Favorites Go to favorites
  Remove from favorites?
  Something went wrong. Please try again later.
  Compare Compare Now
  Product not added for comparison. Please remove any current selection to add this. Manage Selections
  0-10V PIR DROP MT SENSOR BLE 1 2-32V - 20FT LENS - BLACK
  FSP-301B-D-L3-B Wattstopper
  The FSP-3x1B sensors provide continuous dimming light level control based on motion and/or daylight contribution.

  Bazaarvoice SAP Hybris Integration Version 2.8.1

  Other Options Available
  View Details

19 Products available
Sort by:
Compare Products
View:

Types of Light Switches for Residential Lighting Control

Are you familiar with the different types of light switches for the home? Read our guide on the types and best use cases for your lighting control.

Published:Oct, 21, 2024

Wattstopper Architectural Dimming Resources | Legrand

From cutsheets to installation guides, download all your Wattstopper Architectural Dimming resources from one convenient spot!

Corporate Social Responsibility: Legrand presents its new roadmap for 2019-2021

Legrand presents its new roadmap for 2019-2021.

Published:May, 02, 2019

Three Wattstopper® Products Accepted into Prestigious IES 2016 Progress Report | Legrand

San Jose, Calif., October 18, 2016 – Legrand, North America announced today that three Wattstopper products received recognition from the Illuminating Engineering Society (IES) Progress Committee. The Wattstopper DLM 0-10V dimming room controller (LMRC-110 Series), 0-10V dimming wall switch occupancy sensor (DW-311) and Segment Manager 2.1 network controller have been accepted into the 2016 IES Progress Report in the Controls category.

Brand: Wattstopper
Published:Oct, 18, 2016

Legrand Launches Level 2 EV Charger for the Home

Legrand, a longstanding leader in the innovation and manufacture of electrical wiring devices, has announced the launch of their first Electric Vehicle (EV) Charger for residential applications.

Brand: Legrand
Published:Jun, 30, 2023

LFI 2016: Wattstopper DLM Platform Highlights New Features for High Performance Buildings and Advanced Lighting Applications

LFI 2016: Legrand Showcases Code Compliant Control Solutions for Indoor and Outdoor LED Luminaires

Brand: Wattstopper
Published:Apr, 26, 2016

Perspectives on High Performance Building Products | Healthy Materials & Declare Labels | Legrand

The demand for Healthy Materials is a growing trend in the building industry. Learn more on industry initiatives to promote sustainability materials and how Declare Labels supports high performance building certifications like Living Building Challenge.

Brand: Legrand
Published:Dec, 09, 2021

Legrand® Introduces Wattstopper® Blanco LED Light Engines for Tunable White Lighting Solutions | Legrand

Legrand, North & Central America today announced two new tunable white LED light engines, Blanco 2 and Blanco 3, that deliver fixture manufacturers a completely integrated solution that enables the highest quality tunable light available.

Brand: Wattstopper
Published:Aug, 07, 2018

How Much to Install an EV Charger at Home

How much does an EV charging station cost to install? Consider costs like your EV charging level, location and your home’s electrical wiring.

Brand: Pass and Seymour
Published:Nov, 10, 2023

Pennsylvania and City of Philadelphia Adopt New Building Codes for More Energy Efficient Lighting Controls | Wattstopper | Legrand

Pennsylvania is adopting a new energy conservation code effective Oct. 1, 2018 through an update of the Pennsylvania Uniform Construction Code (UCC). The 2015 IECC will be the new building efficiency standard statewide except for in the city of Philadelphia, which is adopting the newer 2018 IECC standard.

Brand: Wattstopper
Published:Aug, 02, 2018

Legrand® Expands Wattstopper® DLM Platform Integration Functionality with New Low-Voltage Auxiliary Devices

Legrand introduced a new low-voltage dual-relay output accessory device and a low-voltage input interface device, both of which extend the capabilities of the Wattstopper® Digital Lighting Management (DLM) system.

Brand: Wattstopper
Published:Dec, 07, 2017

Legrand® Simplifies Human Centric Lighting with New Wattstopper® Tunable Lighting Solutions | Legrand

Legrand, North & Central America and its Eliot Program unveiled its line of Wattstopper Human Centric Lighting (HCL) solutions at LIGHTFAIR International 2017.

Brand: Wattstopper
Published:May, 09, 2017

Control Lighting Using Google Home | Smart Light Switches

Control your Legrand smart light switches in Google Home with voice commands using these step-by-step instructions.

Brand: radiant Collection
Published:Sep, 03, 2025

Create a Custom Light Control with Alexa | Smart Lights

Step-by-step instructions to create custom settings for Netatmo smart lights using Amazon’s Alexa voice commands.

Brand: radiant Collection
Published:Sep, 03, 2025

Nuvo International Distributors | Legrand

To guarantee your Nuvo audio system is tailored to your home, we sell our products through an extensive network of distributors.

How to Choose a Home EV Charger

For anyone making the switch to an electric vehicle (EV), it’s beneficial to understand what to look for in a home EV charger. Here are factors to consider.

Brand: Pass and Seymour
Published:Jun, 28, 2023

Legrand® Launches Wattstopper® Fixture Integrated Outdoor/High Bay Sensors with Bluetooth® Commissioning | Legrand

Legrand® Launches Wattstopper® Fixture Integrated Outdoor/High Bay Sensors with Bluetooth® Commissioning

Brand: Wattstopper
Published:Aug, 09, 2018

Achieving Well-being in High Performance Buildings | Legrand

Credits supporting the well-being and performance building standards: WELL, fitwell, and the Living Building Challenge. Find out how your business cann achieve well-being with Legrand.

Published:Dec, 19, 2023

Sustainability Recognition | Legrand

Legrand is proud to have our commitment to sustainability acknowledged through various journal and magazine articles and other media outlets. We hope you'll enjoy browsing the headlines below and encourage you to click through to read the full articles.

77 Products available
Sort by:
Compare Products
View:

- 1(current)
- 2
- 3

Access Activation Walkerduct BIM Model
BIM Models
zip
Download
Covers Walkerduct BIM Model
BIM Models
zip
Download
Duct Walkerduct BIM Model
BIM Models
zip
Download
Conduit-Adapter Walkerduct BIM Model
BIM Models
zip
Download
Afterset Walkerduct BIM Model
BIM Models
zip
Download
Panel-Connector Walkerduct BIM Model
BIM Models
zip
Download
Elbows Walkerduct BIM Model
BIM Models
zip
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Fiber Loop Kit Installation - 427
Instruction Sheet
pdf
Open PDF
Walker Infloor Systems Trim Plates - 430, 431, 432
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Preset Adapter - S20ADP
Instruction Sheet
pdf
Open PDF
Walkerduct Duct Conduit Hub - D4075
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S3444
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S222
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S3224
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S14
CAD Drawings
dxf
Download
PSRC9 Series Aftersets - 4230
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct - 4240
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct - S224
CAD Drawings
dxf
Download
Walkerduct Variable Offset - 375
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Terrazzo Rings - RTT4,RTT8, RTT13, RTT20
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Adjustable Extension Ring
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Nonmetallic Fittings - S165, S166
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Trim Flange - S125-837PCC
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Communication Cover - 829PFL
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Junction Box Bend Radius Control Inserts Installation
Instruction Sheet
pdf
Open PDF
Walkerduct Pro Series Preset Extensions & Marker Caps - 425, 426, 422RD, 422GR1
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Preset Adapter - S20ADP1, S20ADP2
Instruction Sheet
pdf
Open PDF
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S244
CAD Drawings
dxf
Download
Walkerduct Pro Series Afterset - 4235
CAD Drawings
dxf
Download
Walkerduct/Walkerduct ProSeries Underfloor Duct Support - S3222
CAD Drawings
dxf
Download

- 1(current)
- 2
- 3

Product Availability by Store Location
Hours